|  |  |
| --- | --- |
| Standard ‘grey’ chain: | For fairly stable bottles, moderate speeds, radius max 500 mm, 86 mm wide. |
| Clean room ‘white’ chain: | For fairly stable bottles, moderate speeds, radius max 500 mm, 86 mm wide. Increased wear resistance / reduced dust generation. |
| Standard ‘Green’ chain: | For stable bottles, moderate speeds, radius max 190 mm, 86 mm wide. |
| Stable ‘Black’ chain: | Designed for unstable, difficult bottles, high line speeds, radius min 500 mm, 86 mm wide. |
| Wide Brown chain: | Designed for transport of containers from 10L upwards, 254MM.  Our 86mm range can hold containers up to 5-10L containers, in some cases up to 20L, depending on the container design .  Above the wide chain type is advised. |